**Module 10:**

**infrastructure Security an WAN Technologies –**

***-kumarsinh***

1 - A Cisco Catalyst switch connects to what should be individual user PCs. Each port

has the same port security configuration, configured as follows:

interface range gigabit Ethernet 0/1 - 24

switchport mode access

switchport port-security

switchport port-security mac-address sticky

Which of the following answers describe the result of the port security configuration

created with these commands? (Choose two)

* B. If a user connects a switch to the cable, prevents multiple devices from sending

data through the port.

address into the startup-config

D. Will allow any one device to connect to each port, but will not save that device’s

MAC address into the startup-config

2 - What is the Administrative Distance of internal EIGRP routes?

* B. 90

3 - When a subnet mask is presented in binary, what do the binary 1s represent?

* A. The network portion of an associated address

4 - Which switch would STP choose to become the root bridge in the selection

process?

* A. 32768: 11-22-33-44-55-66ss

5 - Which of the following devices is used by the service provider to provide WAN

Services?

* C. WAN switch

6 - Your Cisco IOS router is

acting as a DHCP server.

Which command will display the addresses that have been handed out to clients on

the LAN?

* D. show ip dhcp bindings

7 - Which of the following commands would you use to enable EIGRP only on those

interfaces with an IP address from 10.1.1.0 through 10.1.1.63?

* A. network 10.1.1.0 0.0.0.63

8 - R3 has a static route configured that points toward the service provider. What

command could you use to have R3 advertise an OSPFv3 default route to the internal

network, regardless of whether R3 had its default static route?

* E. Have R3 use the command default-information originate always in OSPFv3 router

configuration mode.

9 - You are configuring dynamic NAT on your Cisco IOS router. Which command is

used to verify the interfaces that are being used as the outside interface and the

inside interface?

* E. show ip interface

10 - You are configuring dynamic NAT on your Cisco IOS router. Which command is

used to verify the interfaces that are being used as the outside interface and the

inside interface?

* E. show ip interface

11 - When using the “show EtherChannel summary “command, what does the “u “flag

signify?

* D. Unsuitable for bundling

12 - Which command could you enter to encrypt passwords?

* D. All of the above

13 - You are setting up a

Cisco IOS router as a DHCP server.

Which command is used to identify the IPv4 addresses that will be in the DHCP pool?

* F. ip dhcp pool

14 - Which of the following statements are true regarding the processing of ACLs that

have been applied to router interfaces? (Choose two)

🡪 A. Inbound ACLs will be processed before the routing table lookup occurs

C. Outbound ACLs will be processed after the routing table lookup has occurred

15 - imagine you configured OSPFv2 in a small lab network. Which of the following

answers list a condition that could keep the routers in your lab from learning all the

routes to all the IPv4 routes in your small lab network? (Choose two)

🡪 A. An ACL could be blocking router advertisements.

C. Any physical layer problem that would prevent two neighbouring routers from

being able to ping each others IPv4 addresses in the subnet that exists between the

16 - Which statements describe neighbor discovery functionality in IPv6? (Choose two)

🡪 A. Determines the link layer address of a neighbor

D. Queries for duplicate addresses

17 - Which IPv6 prefix will the typical enterprise network receive from the service

provider?

* E. /48

18 - How should be configured a switch so that it could be accessed remotely?

* C. Configure a gateway for the switch

19 - Refer to the exhibit. A network technician is asked to design a small network with

redundancy. The exhibit represents this design, with all hosts configured in the same

VLAN. What conclusions can be made about this design?

🡪 B. Spanning-tree will need to be used.

D. The connection

between switches should be a trunk.